ABBREVIATION   DERIVATION OF ABBREVIATION
  

2DD
  double-side double density

2HD
  double-side high density

3D DDI
  3 Dimensional Device Driver Interface

4GL
  4th generation language

4GT
  4 GB Ram Tuning

A3D
  Aural 3D

ABI
  application binary interface

ABS
  air bearing surface

ACE
  Advanced Computing Environment

ACPI
  Advanced Configuration and Power Interface

ACSM
  Application Control State Machine

ADB
  Apple Desktop Bus

ADE
  automatic design engineering

ADF
  Auto Document Feeder

ADO
  ActiveX Data Objects

ADSI
  Active Directory Service Interfaces

ADT
  attribute definition table

AGP
  Accelerated Graphics Port

AIF
  application integration feature

ALU
  arithmetic logical unit

AML
  ACPI Machine Language

AMR
  Audio/Modem Riser

AOAC
  always on/always connected

API
  application programming interface

APIC
  Advanced Programmable Interrupt Controller

APM
  Advanced Power Management

APNIC
  Asia Pacific Network Information Center

ARC
  Advanced RISC Computing

ASF
  Active Streaming Format

ASL
  ACPI Source Language

ASP
  active server page

ASPI
  Advanced SCSI Programming Interface

ATA
  AT Attachment

ATAPI
  AT Attachment Packet Interface

ATM
  asynchronous transfer mode

ATM API
  asynchronous transfer mode application programming interface

ATMS
  Automated Traffic Management Systems

AT-UD
  Unimodem Diagnostics Command

ATX
  AT eXtension

AUI
  Attachment Unit Interface

AVGA
  Advanced VGA

AVI
  Audio Visual Interleaving

AWT
  Abstract Window Toolkit

BAR
  base address register

BASIC
  beginner's all-purpose symbolic instruction code

BBS
  bulletin board system

bcc
  blind carbon copy

BCL
  bias compensation layer

BDA
  BIOS Data Area

BDC
  backup domain controller

BDK
  Business Development Kit

BIOS
  basic input/output system

BIPS
  billion instructions per second

BIS
  boot integrity services

BLOB
  Binary Large Object

BML
  Broadcast Markup Language

BMP
  Basic Multilingual Plane

BMP
  Bit Map

BMS
  broadcast message server

BNF
  Backup Naur Form

BOF
  beginning of file

BOOTP
  bootstrap protocol

BPB
  BIOS Parameter Blocks

BPC
  Broadcast PC

BPI
  bit per inch

BPI
  bit per instruction

bpp
  bits per pixel

BPR
  business process reengineering

bps
  bit per second

BRAN
  Broadband Radio Access Networks

BRI
  Basic Rate Interface

BSDL
  Boundary Scan Description Language

BTL
  backplane transceiver logic

BTRON
  Business TRON

BUS
  broadcast unknown server

C&C
  computer and communication

CA
  conditional access

CA
  certification authority

CAD
  computer aided design

CAD/CAM
  computer aided design / computer aided manufacturing

CAE
  computer aided engineering

CAE
  common application environment

CAE
  Conditional Access Engine

CAI
  computer assisted (aided) instruction

CAL
  common application language

CAL
  computer assisted learning

CALS
  Computer-aided Acquisition and Logistical Support

CAM
  computer aided manufacturing

CAM
  content addressable memory

CAPI
  Cryptographic API

CASE
  computer aided software engineering

CAT
  computer aided testing

CBQ
  class-based queuing

CDA
  Compound Document Architecture

CDB
  Command Description Block

CDC
  Connected Device Configuration

CDDI
  copper distributed data interface

CDE
  Common Desktop Environment

CDF
  Channel Definition Format

CDFF
  Common Document File Format

CDIF
  Common Document Intermediate Format

CDL
  Class Definition Language

CDP
  Concept Description Plan

CDRA
  Character Data Representation Architecture

CDSA
  Common Data Security Architecture

CEDR
  Windows CE Driver Repository

CG
  computer graphics

CGA
  Color Graphics Array

CGA
  column grid array

CGI
  Computer Graphics Interface

CGI
  common gateway interface

CGM
  Computer Graphics Metafile

CHRP
  Common Hardware Reference Platform

CHS
  cylinder head sector

CI
  Component Instrumentation

CICS
  Customer Information Control System

CID
  Compatible ID

CIFS
  Common Internet File System

CIM
  computer integrated manufacturing

CIM
  Common Information Model

CIMOM
  CIM Object Model

CINF
  check (modem) INF tool

CIS
  card information structure

CIS
  customer information system

CISC
  complex instruction set computer

CL
  CAS(column address strobe) Latency

CLAD
  cell assembler/disassembler

CLDC
  Connected Limited Device Configuration

CLI
  Call Level Interface

CLOS
  Common Lisp Object System

CLP
  cell loss priority

CLUT
  Colour Look-Up Table

CMC
  Computer Numeric Control

CMIP
  common management information protocol

CML
  Caucus Markup Language

CMM
  color matching modules

CMM
  Capability Maturity Model

CNR
  Communication and Networking Riser

COBOL
  common business oriented language

COCOMO
  construction cost model

COM
  Component Object Model

CORBA
  Common Object Request Broker Architecture

COSE
  Common Open Software Environment

COSS
  Common Object Service Specification

CP/M
  control program for a microcomputer

CPN
  central processing node

CPU
  central processing unit

CRL
  Certificate Revocation List

CSEL
  Cable SELect

CSMA/CA
  carrier sense multiple access with collision avoidance

CSMA/CD
  carrier sense multiple access with collision detection

CSN
  Card Select Number

CSS
  Contact Start Stop

CSV
  comma separated value format

CT
  computerized tomography

CTI
  Computer Telephony Integration

CTRON
  central-TRON

CTS
  computerized typesetting system

CTS
  Clear To Send

DA
  data administrator

DAA
  Data Access Arrangement

DAC
  Design Automation Conference

DAP
  Directory Access Protocol

DAS
  dual attachment station

DASD
  direct access storage device

DB
  database

DB2
  Database 2

DBA
  database administrator

DBC
  Device Bay Controller

DBM
  Dual Bit Map

DBMS
  database management system

DC
  device context

DCD
  Data Carrier Detect

DCE
  Data Communications Equipment

DCE
  distributed computing environment

DCF
  Distributed Coordination Function

DCI
  display control interface

DCL
  Delay Calculation Language

DCLZ
  data compression Lempel-Ziv

DCOM
  Distributed Component Object Model

DDC2B
  Display Data Channel Standard, Level 2B

DDE
  Dynamic Data Exchange

DDF
  Data Description Field

DDFF
  Distributed Disk File Facility

DDK
  Driver Developers Kit

DDL
  data definition language

DDM
  design data manager

DDM
  Distributed Data Management

DDML
  Display Driver Management Layer

DDoS
  distributed denial of service

DDS
  Digital Data Storage

DDS
  Distributed Data Server

DEF
  Design Exchange Format

DES
  data encryption standard

DFM
  Distributed File Management

DFS
  Distributed File System

DFT
  Drive Fitness Test

DFT
  design for test

DIB
  Device Independent Bitmap

DIB
  Directory Information Base

DIFS
  distributed access inter frame space

DIM
  Device Interface Module

DINA
  Distributed Information Processing Network Architecture

DIPS
  Dendenkousha Information Processing System

DISA
  Distributed Information Processing System Architecture

DISM
  Digital Interface Standards for Monitor

DISP
  Directory Information Shadowing Protocol

DIT
  Directory Information Tree

DLC
  data link control

DLCI
  datalink channel identifier

DLL
  dynamic link library

DME
  Distributed Management Environment

DMI
  Desktop Management Interface

DML
  data manipulation language

DMTF
  Desktop Management Task Force

DMWG
  Data Management Work Group

DN
  Distinguished Name

DNS
  Domain Name System

DOA
  data oriented approach

DOM
  Distributed Operations Master

DOMF
  Distributed Object Management Facility

DOP
  Directory Operational Protocol

DOS
  Disk Operating System

DP
  data parallelism

DPC
  Deferred Procedure Call

DPI
  dot per inch(dpi)

DPMI
  DOS protected mode interface

DPMS
  Display Power Management Signaling

DRC
  design rule checker

DRDA
  Distributed Relational Database Architecture

DRF
  Data Recovery Field

DRM
  Digital Rights Management (System)

DR-PI
  design representation programming interface

DS
  Directory Service

DSA
  Digital Signature Algorithm

DSE
  Development Software Engineer

DSM
  digital storage media

DSM-CC
  digital storage media-control command

DSO
  Dynamic Shared Object

DSS
  Microsoft Mail Directory Synchronization (dir-sync) Server

DSS
  decision support system

DSSSL
  Document Style Semantics and Specification Language (ISO/IEC 10179)

DSU
  digital service unit

DTC
  Distributed Transaction Coordinator

DTD
  document type definition

DTE
  data terminal equipment

DTM
  data transfer mechanism

DTP
  desktop publishing

DTR
  Data Terminal Ready

DVMCI
  digital video media control interface

DVO
  Digital Video Output

DXF
  drawing interchange file

EA
  extended attributes

EAB
  embedded array block

EAP
  Extensible Authentication Protocol

EASI
  embedded all-in-one system interface

EBCDIC
  extended binary coded decimal interchange code

EBCOT
  Embedded Block Coding with Optimized Truncation

EDA
  electronic design automation

EDD
  Enhanced Disk Drive

EDF
  earliest deadline first

EDI
  electronic data interchange

EDID
  Extended Display Identification Data

EDIF
  electronic design interchange format

EDO
  extended data out

EDP
  electronic data processing

EEMBC
  EDN Embedded Microprocessor Benchmark Consortium

EFS
  Encrypting File System

EGA
  Extended Color Graphics Array

EGA
  Enhanced Graphics Adapter

EHCI
  Enhanced Host Controller Interface

EHLLAPI
  extended high level language application programming interface

EIDE
  Enhanced Integrated Device Electronics

EIO
  Extended I/O

EISA
  extended industry standard architecture

ELF
  Extended Link Format

EM
  electronic mail

EMB
  Extended Memory Block

EMC
  electro magnetic compatibility

EMF
  Extended metafile

EMM
  Entitlement Management Messages

ENIAC
  Electronic Numerical integrator And Calculator

EOF
  end of file

EPIC
  Explicitly Parallel Instruction Computing

EPP
  Enhanced Parallel Port

E-R
  entity-relationship

ERC
  electrical rule checking

ERP
  Error Recovery Procedure

ES
  expert system

ESA
  extended service area

ESA
  Enterprise Systems Architecture

ESC/P
  Epson Standard Code for Printer

ESCD
  Extended System Configuration Data

ESCON
  enterprise systems connection

ESDI
  enhanced small device interface

ESIOP
  environment-specific inter-ORB protocol

ESS
  extended service set

ETK
  Embedded Toolkit

EUC
  Extended UNIX Code

EUC
  end-user computing

EUI-64
  Extended Unique Identifier

EVC
  Enhanced Video Connector

EWS
  engineering workstation

ExCA
  Exchangeable Card Architecture

FACS
  Firmware ACPI Control Structure

FAPI
  Fingerprint Aware Application Program Interface

FAT
  file allocation table

FBAPI
  Fingerprint Basic Aware Application Program Interface

FCA
  Fibre Channel Association

FC-AL
  Fibre Channel Arbitrated Loop

FCB
  file control block

FC-EP
  Fibre Channel Extended Physical

FCP
  Fibre Channel Protocol

FCP
  function control protocol

FC-PH
  Fibre Channel Physical

FCS
  frame check sequence

FCSI
  Fibre Channel Systems Initiative

FD
  floppy disc

FDC
  Floppy Disk Drive Controller

FDD
  floppy disc drive

FDDI
  Fiber Distributed Data Interface

FDIV
  Floating (point) Divide

FDL
  Facility Data Link

FDO
  Functional Device Object

FE
  Framing Error

FEAPI
  Fingerprint Extended Aware Application Program Interface

FFOL
  FDDI Follow on LAN

FHN
  Fiber HUB Node

FiDO
  Filter Device Object

FIM
  Function Component Interface Module

FIQ
  Fast Interrupt reQuest

FLP
  fast link pulse

FMV
  Full Motion Video

FMV
  fair market value

FNA
  Fujitsu Network Architecture

FNO
  Foreign Namespace Object

FoIP
  FAX over Internet Protocol

FORTRAN
  formula translator

FP
  function point

FPA
  function point analysis

FPU
  floating-point processing unit

FR
  frame relay

FRS
  File Replication Service

FSB
  Front Side Bus

FSD
  File System Driver

FSF
  free software foundation

FSRTL
  File System Run Time Library

FTAM
  File Transfer, Access and Management

FTC
  fault tolerant computer

FTP
  File Transfer Protocol

FTS
  fault tolerant system

FTTB
  fiber to the building

FTTC
  fiber to the curb

GART
  Graphic Address Re-mapping Table

GCP
  Global Computation Platform

GDA
  Global Document Annotation

GDI
  Graphical Device Interface

GDT
  Global Descriptor Table

GFC
  Generic Flow Control

GIDEI
  General Input Device Emulation Interface

GIF
  Graphics Interchange Format

GINA
  Graphical Identification and Authentication

GKS
  Graphical Kernel System

GMR
  giant magnetoresistive

GNU
  general public license

GNU
  GNU's Not Unix, "guh-NEW"

GPC
  Graphics Performance Characterization

GPIB
  general purpose interface bus

GPIO
  General Purpose I/O

GPL
  GNU Public License

GSS-API
  Generic Security Service Application Program Interface

GTF
  Generalized Timing Formula

GVIF
  Gigabit Video Interface

H/W
  hardware

HA
  home automation

HAA
  Hitachi Application Architecture

HAMR
  Heat Assisted Magnetic Recording

HCI
  Host controller Interface

HCL
  Hardware Compatibility List

HDA
  head disk assembly

HDC
  hard disk controller

HDCG
  high definition computer graphics

HDD
  hard disk drive

HDL
  hardware description language

HDLC
  High Level Data Link Control procedures

HDT
  Host Digital Terminal

HEC
  Header Error Control

HEL
  hardware emulator layer

HFS
  hierarchical file system

HID
  Human Interface Device

HIPPI
  high performance parallel interface

HLLAPI
  high-level language application programming interface

HMA
  high memory area

HMI
  Human Machine Interface

HPC
  high performance computation

HPCCI
  High-performance Computing and Communications Initiative

HPF
  High Performance Fortran

HPFS
  High Performance File System

HRTF
  Head Related Transfer Function

HSFS
  High-Sierra File System

HSM
  Hierarchical Storage Management

HSSI
  High-Speed Serial Interface

HSTP
  High Speed Transport Protocol

HTPC
  Home Theater Personal Computers

I2O
  Intelligent Input/Output

IA-PC
  Intel Architecture Personal Computer

IBIS
  I/O buffer information specification

ICC
  integrated communication controller

ICCCM
  Inter-Client Communication Conventions Manual

ICM
  Image Color Management

ICM
  Image Compression Manager

ICU
  ISA Configuration Utility

IDAPI
  Integrated Database API

IDE
  integrated device electronics

IDL
  Interface Definition Language

IDM
  Interleaved Device Mode

IDT
  Internet Development Toolbox

IDT
  Interrupt Dispatch Table

IE
  Internet Explorer

IF
  Implements Forum

IFC
  internet foundation class

IFS
  ICOT Free Software

IFS
  instable file system

IFSMGR
  Instable File System Manager

IGES
  Initial Graphics Exchange Specification

IHV
  independent hardware vendor

IME
  Input Method Editor

IN
  intelligent network

Indeo
  Intel Video Technology

INN
  InterNetNews

IOOM
  the Ithaca Object-Oriented Methodology

IOS
  I/O Supervisor

IP
  interface protocol

IPC
  interprocess communication

IPD
  Integrated Program Decoder

IPI
  Intelligent Peripheral Interface

IPL
  Initial Program Load

IrLAP
  infrared link access protocol

IrLMP
  infrared link management protocol

IrMC
  Infrared Mobile Communications

IrOBEX
  Infrared Object Exchange Protocol

IRP
  I/O Request Packet

IRQ
  interrupt request

IrTA
  infrared terminal adapter

IrTran-P
  Infrared Transfer Picture

IrWW
  Infrared Wrist Watch

ISA
  Industry Standard Architecture

ISAPI
  information server API

iSCSI
  Internet SCSI (SCSI over TCP/IP)

ISIS
  Image and Scanner Interface Specification

IS-IS
  Intermediate System to Intermediate System Infra Domain Routing Exchange


  Protocol

ISM
  Interface Subscriber Module

ISO/OSI
  International Standards Organization Open System Interconnection

ISR
  Interrupt Service Routine

IST
  interrupt service thread

ISV
  independent software vendor

IT
  information technology

ITRON
  Industrial TRON(The Realtime Operating system Nucleus)

IVD LAN
  integrated voice and data LAN

IVV
  Independent Verification & Validation

IX
  internet exchange

IXC
  Inter Exchange Carrier

JAIN
  Integrated Network APIs for the Java Platform

JAM
  Java administration server

JAR
  Java archive

Java VM
  Java Virtual Machine

JCL
  job control language

JCP
  Java Community Process

JFC
  Java Foundation Classes

JIT
  Just-In-Time

JLE
  Japanese Language Environment

JNI
  Java Native Method Interface

JOIS
  JICST On-line Information System

KBM
  knowledge based machine

KCC
  Knowledge Consistency Checker

KDD
  Knowledge Discovery in Databases

KDT
  keyboard definition table

KPA
  key process area

KPS
  key predistribution system

LA
  laboratory automation

LAN
  local area network

LAPM
  Link Access Protocol, Modem

LBA
  logical block address

LBP
  laser beam printer

LCC
  levelized compiled code

LCF
  Link Control Facility

LDAP
  lightweight directory access protocol

LDI
  LVDS Display Interface

LEC
  LAN emulation clients

LECS
  LAN emulation configuration server

LES
  LAN emulator server

LFN
  long file name

LIM
  Lotus-Intel-Microsoft

LIP
  Loop Initialization Primitive

LP
  laser printer

LPC
  Low Pin Count

LPE
  layout parameter extraction

lpi
  line per inch

LPT
  line printer

LSSD
  level sensitive scan design

LSTF
  least slack time first

LU
  Logical Unit

LUN
  logical unit number

LVE
  Live Video Extensions

LVM
  logical volume manager

MA
  message area

MAC
  media access control

MADK
  Microsoft ActiveX Development Kit

MAOS
  multi application operating system

MAPI
  Messaging Application Programming Interface

MAS
  multiple-address space

MBONE
  multicast backbone

MCA
  multi-channel access

MCA
  Micro Channel Architecture

MCD
  Mini Client Driver

MCGA
  Multi Color Graphics Array

MCI
  Media Control Interface

MCI
  Multimedia Control Interface

MCT
  Modem Compatibility Test

MCU
  multipoint connection unit

MDD
  multi-valued decision diagram

MDI
  Multiple Document Interface

MDK
  Modem Developers Kit

MDL
  memory descriptor list

MESN
  Media Event Status Notification

MF
  more fragments (bit)

MF
  media flexible

MFP
  multi-function peripheral

MFT
  master file table

MHS
  message handling system

MI
  Management Interface

MIA
  Multivendor Integrated Architecture

MIDI
  musical instrument digital interface

MIDP
  Mobile Information Device Profiles

MIF
  Management Information File

MIF
  management information format

MII
  media independent interface

MIMD
  multiple instruction stream multiple data stream

MIPS
  million instructions per second

MIS
  management information system

MMC
  Microsoft Management Console

MMHID
  Multimedia Human Input Device

MMIO
  memory-mapped I/O

MMU
  memory management unit

MMX
  multimedia extension

MNLS
  Multi National Language Support

MNP
  Microcom Networking Protocol

MOD
  movie on demand

MOF
  Management Object Format

MOLAP
  multi-dimensional online analytical processing

MOM
  message oriented middleware

MOOD
  Methodology for Object Oriented Design

MP/M
  multi-programming monitor

MPC
  Multimedia Personal Computer

MPDU
  MAC Protocol Data Unit

MPI
  Message Passing Interface

MPIC
  Multiprocessor Interrupt Controller

MPPE
  Microsoft Point-to-Point Encryption

MPS
  MultiProcessor Specification

MR
  Mixed Reality

MRCI
  Microsoft Real-time Compression Interface

MSCDEX
  Microsoft CD-ROM Extensions

MSCS
  Microsoft Cluster Server

MSDL
  Microsoft Download Library

MSDN
  Microsoft Developer Network

MS-DOS
  Microsoft disk operating system

MSDU
  MAC Service Data Unit

MSEN
  Media Status Event Notification

MSMQ
  Microsoft Message Queue Server

MSO
  multiple system operator

MTD
  Memory Technology Driver

MTE
  Message Transfer Element

MTF
  Microsoft Tape Format

MTS
  Microsoft Transaction Server

MTU
  maximum transmission unit

MTU
  Maximum Transfer Unit

MUD
  Master User Domain

MUI
  multimedia user interface

MULTOS
  multiapplication operating system

MVEX
  Minimal Video Extension to X

MVS
  Multiple Virtual Storage

MVS/ESA
  MVS/Enterprise Systems Architecture

NABTS
  North American Basic Teletext System

NAPLPS
  North American Presentation-Level-Protocol Syntax

NBDD
  NetBIOS datagram distribution server

NBNS
  NetBIOS name server

NC
  naming context

NC
  Network Computer

NCB
  network control block

NCP
  Netware Core Protocol

NCRP
  Network Computer Reference Specification

NCS
  Network Computing System

NCSS
  non-comment source statements

NCU
  network control unit

NDD
  Norton Disk Doctor

NDIS
  Network Driver Interface Specification

NDPS
  network distributed print system

NDS
  Netware Directory Service

NDS
  Novell Directory Service

NEEDS
  Nikkei Economic Electronic Databank System

Net PC
  network personal computer

NetBEUI
  NetBIOS Extended User Interface

NETBIOS
  Network Basic Input/Outputs System

NFS
  network file system

NGIO
  Next Generation Input/Output

NIC
  network interface card

NIT
  Network Information Table

NIU
  Network Interface Unit

NLM
  NetWare loadable module

NLS
  national language support

NNI
  network node interface

NOD
  News on Demand

NOI
  Notice Inquiry

NOS
  Network Operating System

NPI
  Network provider Interface

NPR
  Notice of Proposed Rulemaking

NREN
  National Research and Education Network

nrt
  non-real-time

NSP
  native signal processing

NT
  New Technology

NT
  Network Termination

NTDS
  Windows NT Directory Service

NTFS
  NT File System

NTLM
  Windows NT LAN Manager

NTP
  Network Time Protocol

NTS/E
  Windows NT Server, Enterprise Edition

NVOD
  Near Video on Demand

OADG
  Open Architecture Developing Group

OAK
  OEM Adoption Kit

OAM
  operation and maintenance

OCMP
  Open Computing environment for MIPS Platform

OCN
  Open Computer Network

OCX
  OLE Custom control

ODA
  Open Document Architecture

ODAPI
  Open Database Application Programming Interface

ODB
  object-oriented database

ODBC
  Open Database Connectivity

ODBMS
  object(-oriented) database management system

ODI
  Open Datalink Interface

ODS
  operational data store

ODSI
  Open Directory Services Interface

OEX
  OLE System Control

OFS
  Object File System

OGI
  Open Graphics Initiative

OHCI
  Open Host Controller Interface

OID
  Object ID

OLAP
  on-line analytical processing

OLCP
  on-line complex processing

OLE
  Object Linking & Embedding

OLTP
  on-line transaction processing

OMA
  Object Management Architecture

OMAP
  Open Multimedia Application Platform

OMG-IDL
  Object Management Group Interface Definition Language

OMG-UNO
  Object Management Group Universal Networked Objects

OMT
  Object Modeling Technique

ONC
  Open Network Computing

ONP
  open network provision

ONU
  optical network unit

OOA
  object-oriented analysis

OOAD
  object-oriented analysis and design

OOD
  object-oriented design

OODB
  object-oriented database

OOP
  object-oriented programming

OOPS
  object-oriented programming system

OOPSLA
  Object-Oriented Programming, Systems, Languages, and Application

OpenHCI
  Open Host Controller Interface

OPK
  OEM preinstallation kit

OQL
  object query language

OR
  operations research

ORB
  Operation Request Block

ORB
  Object Request Broker

ORDB
  Object-Relational Database

OS
  operating system

OSA
  Open Scripting Architecture

OSF
  Open Software Foundation

OSI
  Open System Interface

OSI
  Open Systems Interconnection

OSPM
  OS-directed Power Management

OSR
  OEM service release

OTG
  on the go

OTS
  Object Transaction Service

OVI
  Open Verilog International

PA
  Precision Architecture

PABX
  private automatic branch exchange

PAC
  Privilege attribute Certificate

PAD
  Program associated data

PAD
  packet assembler/disassembler

PAD
  Problem Analysis Diagram

PARCOR
  partial auto correlation

PA-RISC
  Precision Architecture-RISC

PAS
  Pre-Boot Authentication Service

PC
  personal computer

PC
  packet classifier

PC-DOS
  Personal Computer-Disk Operating System

PCI
  Peripheral Component Interconnect

PCI PM
  PCI Bus Power Management Specification

PCIC
  PC Card I/O Cards

PCP
  Printer Control Protocol

PCS
  physical coding sublayer

PCT
  Private Communication Technology

PCTE
  portable common tool environment

PDA
  personal digital assistants

PDC
  primary domain controller

PDC
  Program Delivery Control

PDC
  professional developers conference

PDEF
  physical design exchange format

PDF
  Portable Document File

PDK
  Peripheral Developers Kit

PDL
  Process Design Language

PDL
  page description language

PDM
  product data management system

PDM
  Primary Defect Map

PDO
  physical device object

PDQ
  parallel data query

PDS
  public domain software

PEX
  PHIGS Extension to X

PFS
  Product Functional Specification

PGP
  pretty good privacy

PHIGS
  Programmer's Hierarchical Interactive Graphics System

PIAM
  Platform Independent Application Model

PIC
  Personal Intelligent Communicator

PIC
  Programmable Interrupt Controller

PICS
  Platform for internet Content Selection

PID
  Program ID

PID
  packet identification

PIF
  program information file

PIM
  Parallel Inference Machine

PIO
  programmed input/output

PIP
  P Internet Protocol

PIT
  Programmable Interrupt Timer

PKT
  Partition Knowledge Table

PL/1
  Programming Language one

PLB
  Picture Level Benchmark

PLDA
  Private Loop Direct Attach

PLI
  programming language interface

PMA
  physical medium attachment

PMC
  PCI Mezzanine Card

PMD
  physical medium dependent

PMD
  physical media dependent sublayer

PME
  Power Management Event

PML
  Physical Markup Language

PNG
  Portable Network Graphics

POI
  point of interface

POP
  point of presence

POP
  post office protocol

POPS
  peta operations per second

POSIX
  portable operating system interface

POST
  power-on self-test

POWER
  Performance Optimization with Enhanced RISC

pp
  program parallelism

ppm
  pages per minute

PPP
  Point-to-Point Protocol

PPTP
  point-to point tunneling protocol

PRM
  Performance Report Message

PS/2
  personal system/2

PS2
  Play Station 2

PSS
  Product Support Services

PSW
  Program Status Word

PVC
  permanent virtual circuit

PVM
  Parallel Virtual Machine

PVP
  Packet Video Protocol

QBE
  query by example

QCELP
  Qualcomm code excited linear prediction

QCIF
  quarter common intermediate format

QIC
  Quarter-inch Cartridge

QRSL
  Quad Rambus Signal Level

QTVR
  QuickTime VR

QVGA
  quarter video graphic array

RAD
  rapid application development

RAID
  Redundant Arrays of Inexpensive Disks

RAW
  read and write

RDA
  remote database access

RDB
  relational database

RDBMS
  relational database management system

RDN
  Relative distinguished Name

RFID
  Radio Frequency Identification

RFT:DCA
  Revisable From Text : Document Content Architecture

RID
  Relative ID

RIFF
  Resource Interchange File Format

RIMM
  Rambus Inline Memory Module

RIPL
  Remote Initial Program Load

RISC
  reduced instruction set computer

RLC
  Run Length Coding

RMI
  remote method invocation

RNI
  Raw Native Interface

ROLAP
  Relational online analytical processing

RPC
  remote procedure call

RPE-LTP
  Regular Pulse Excitation-Long Term Predictive cording

RPG
  Report Program Generator

RSL
  Rambus Signal Level

RSX
  Intel Realistic Sound eXperience

RT
  remote terminal

RT
  Real-Time

RTC
  real-time clock

RTF
  Rich Text Format

RTK
  real time kinematic

RTOS
  Real Time Operating System

RTS
  Request To Send

RWS
  Remote Winsock

S/PDIF
  Sony Philips Digital Interface

S/W
  software

SA
  Structured Analysis

SAA
  Systems Application Architecture

SACCH
  slow associated control channel

SAF
  synthetic antiferromagnet

SALT
  Speech Application Language Tag

SAM
  SCSI-3 Architecture Model

SAP
  secondary audio programming

SAR
  segmentation and reassembly

SASI
  Shugart Associates System Interface

SBC
  surrounded by complement

SBC
  SCSI-3 Block Commands

SBE
  software behavior estimation

SBP
  Serial Bus Protocol

SBS
  Smart Battery Specification

SBS
  Smart Battery Systems

SC
  Structured Chart

SCA
  single connector attachment for SCSI Disk Drives

SCAM
  SCSI Configured Automatically

SCD
  SPARC Compliance Definition

SCI
  scaleable coherent interface

SCID
  Service Channel ID

SCM
  Software Configuration Management

SCP
  Source Compatibility Package

SCP
  Service Control Point

SCSI
  small computer system interface

SCSIFCP
  SCSI Fibre Channel Protocol

SCSL
  Sun Community Source License

SCT
  Software Compatibility Test

SD
  Structured Design

SD
  shared disk

SDAS
  System Development Architecture & Support facilities

SDE
  Software Development Engineer

SDH
  synchronous digital hierarchy

SDK
  software developer's kit

SDLC
  Synchronous Data Link Control

SDP
  session description protocol

SDR
  Sustained Data Rate

SDU
  Service Data Unit

SE
  system engineer

SE
  shared everything

SECC
  Single Edge Contact Cartridge

SECE
  secure electronic commerce environment

SES
  solution exchange standard

SETP
  Stream Environment Transport Protocol

SFF
  Small Form Factor

SFN
  single frequency network

SFS
  stick-on free slider

SFS
  Shared File System

SGML
  Standard Generalized Markup Language

SI
  Service Information

SI
  system integration

SID
  Subsystem ID

SIE
  Serial Interface Engine

SIMD
  single instruction stream-multiple data stream

SIPC
  Simply Interactive Personal Computer

SIR
  serial infrared interface

SIS
  strategic information system

SLCP
  Software Life-Cycle Processes

SLIC
  subscriber line interface circuit

SLIP
  Serial Line IP

S.M.A.R.T.
  Self-Monitoring, Analysis and Reporting Technology

SMB
  server message block

SMBus
  System Management Bus

SMDL
  Standard Music Description Language

SMI
  system management interrupt

SMM
  system management mode

SMS
  system management server

SNA
  Systems Network Architecture

SNA
  Software Network Architecture

SOF
  start of frame

SPA
  Software Process Assessments

SPARC
  Scalable Processor Architecture

SPDL
  Standard Page Description Language

SPEF
  Standard Parasitic Exchange Format

SPF
  standard parasitic format

SPI
  Serial Peripheral Interface

SPICE
  Simulation Program with Integrated Circuit Emphasis

SPID
  Service Profile Identifier

SPMD
  single program multiple data stream

SPS
  Shock Protection System

SPSR
  Stored Program Status Register

SPX
  Sequenced Packet Exchange

SQL
  structured query language

SRB
  Stream Request block

SRC
  sample rate converter

SRC
  sampling rate change

SSA
  Serial Storage Architecture

SSADM
  Structured Systems and Design Method

SSC
  Smart Signal Conditioning

SSDP
  Simple Service Discovery Protocol

SSI
  single system image

SSL
  Secure Socket Layer

SSP
  serial storage protocol

SSPI
  Security Support Provider Interface

SSTF
  shortest seek time first

SSTV
  slow scan television

STD
  State Transition Diagram

STEP
  Standard for the Exchange of Product

STI
  Still Image architecture

STT
  Secure Transaction Technology

SVC
  switched virtual connection

SVG
  Scalable Vector Graphics

SVGA
  super video graphics array

SVID
  System Vendor Interface Definition (IDentification)

SXGA
  super extended graphic array

SXVGA
  super extended video graphics array

TAPI
  Telephony application programming interface

TBI
  Ten Bit Interface

TCL
  Tool command Language

TD-CDMA
  time division-code division multiple access

TDE
  telephone data entry

TDI
  Transport Driver Interface

TE
  terminal equipment

TFTP
  trivial file transfer protocol

TIFF
  Tagged Image File Format

TLD
  Top Level Domain

TLI
  Transport Level Interface for UNIX

TM
  transaction manager

TMDS
  Transition Minimized Differential Signaling

TMF
  transaction monitoring facility

TOC
  table of contents

TREC
  Texture and Rendering Engine Compression

TRON
  The Realtime Operating system Nucleus

TSD
  type-specific driver

TSR
  terminate-and-stay-resident

TSS
  time sharing system

TWAIN
  Technology Without Any Interested Name

TwinVQ
  transform domain weighted interleave vector quantization

TXD
  Transmission Data

UAS
  User Account System

UBR
  unspecified bit rate

UCT
  Universal Coordinate Time

UDL/I
  unified design language of integrated circuit

UDP
  User Datagram Protocol

UFS
  UNIX file system

UHCI
  Universal Host Controller Interface

UI
  UNIX International

UI
  User Interface

UI
  Unit Interval

UIMS
  user interface management system

ULP
  upper layer protocol

UML
  unified modeling language

U-N
  User to Network primitive

UNC
  Universal Naming Convention

UNI
  user network interface

UP
  Uniprocessor

UPC
  Usage Parameter Control

UPF
  Uni Picture Format

URB
  USB request block

URL
  Uniform Resource Locator

USB
  Universal Serial Bus

USN
  Update Sequence Number

UTMI
  USB2.0 Transceiver Macrocell Interface

UTOPIA
  Universal Test & Operations PHY Interface for ATM

U-U
  User to User primitive

UUCP
  UNIX to UNIX Copy Program

UVGA
  Ultimate VGA (1024 x 768, 60fps)

VAFC
  Vesa Advanced Feature Connector

VAN
  value added network

VB
  Visual Basic

VBA
  Microsoft Visual Basic Programming System Application Edition

VBE
  VESA BIOS Extension

VBX
  Visual Basic Extension

VC
  virtual channel

VC
  virtual circuit

VCCI
  Voluntary Control Council for Interference by Data Processing Equipment


  and Electronic Office Machines

VCDFSD
  Virtual CD-ROM File System Driver

VCI
  Virtual Channel Identifier

VDD
  Virtual Device Driver

VDD
  Version Description Document

VDIF
  Video display Information Format

VDM
  Virtual DOS Machine

VDM
  Virtual Device Manager

VDMA
  Virtual DMA

VDMAD
  Virtual DMA Device

VDO
  Video Distribution Office

VDP
  video datagram protocol

VDS
  Virtual DMA Services

VDT
  video display terminal/visual display terminal

VESA
  Video Electronics Standard Association

VFS
  virtual file system

VFW
  Video for Windows

VGA
  Video Graphics Array

VHDL
  VHSIC hardware description language

VI
  VHDL International

VIP
  Video Information Provider

VISCA
  Video System Control Architecture

VITAL
  VHDL Initiative toward ASIC Libraries

VL-Bus
  VESA local bus

VLM
  Very Large Memory

VM
  Virtual Machine

VM/CMS
  Virtual Machine / Conversational Monitor System

VM/ESA
  Virtual Machine/Enterprise Systems Architecture

VME
  versa module European

VMS
  Virtual Memory System

VMTP
  Versatile Message Transaction Protocol

VOD
  video-on-demand

VP
  virtual path

VPE
  Video Port Extension

VPI
  virtual path identifier

VpicD
  virtual programmable interrupt controller device

VRML
  virtual reality modeling language

VSAM
  virtual storage access method

VSD
  Vendor Specific Driver

VUDA
  VESA Unified Graphic Architecture

VUMA
  VESA Unified Memory Architecture

VVIDD
  VESA Video Interface for Digital Display

VxD
  Virtual Device Driver

VXI
  VMEbus extensions for instrumentation

WAIS
  wide area information server

WBMP
  Wireless Bitmap

WBS
  work breakdown structure

WBT
  Windows-Based Terminal

WC
  write combining

WCEfA
  Windows CE for Automotive

WD
  working draft

WDCTRL
  Western Digital-Compatible Hard Disk Controller

WDI
  Watchdog input

WDL
  Windows Driver Library

WDM
  Win32 Driver Model

WDMCSA
  WDM Connection and Streaming Architecture

WHIIG
  Windows Hardware Instrumentation Implementation Guideline

WHQL
  Windows Hardware Quality Laboratory

WIA
  Windows Image Acquisition

WIA
  Wearable Internet Appliance

WIDE
  Widely Integrated Distributed Environment

WIFE
  Windows Intelligent Font Environment

WinHEC
  Windows Hardware Engineering Conference

WINNLS
  Windows National Language Support

WINS
  Windows Internet Name Service

WinSock
  Windows Sockets 2.0

WIPS
  whetstone instructions per second

WLL
  wireless local loop

WMA
  Windows Media Audio

WMF
  Windows Meta-File

WMI
  Windows Management Instrumentation

WORM
  write once, read many

WOSA
  Windows Open System Architecture

WPS
  Windows Printing System

WRAM
  Window RAM

WRB
  Web Request Broker

WS
  workstation

WSH
  Windows Scripting Host

WSP
  WinSock Proxy

WSS
  Windows Sound System

WWDU
  Work With Display Units

XCOFF
  eXtended Common Object File Format

XDR
  external data representation

XFN
  X/Open Federated Naming

XGA
  eXtended Graphics Array

XHTML
  eXtensible Hypertext Markup Language

XIMP
  X Window System Input Method Protocol

XIP
  eXecute-in-Place

XKP
  Extended Kanji Processing

XMS
  eXtended Memory Specification

XNS
  Xerox Network System

XPC
  extended processing complex

XPG
  X/Open Portability Guide

XTP
  express Transfer Protocol

Y2K
  Year 2000

ZAK
  Zero Administration Kit foe Windows NT Workstation

ZAW
  Zero Administration Windows

ZIP
  Zone Improvement Plan

ZM
  zone marker

ZTAT
  Zero Turn Around Time

ZVP
  Zoomed Video Port
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